Canlift CL-07



**CL-07
Lift Landing Door Retering Cam**

 **»** High quality and with technical features,

**»** Convenient assembly and hardness,

**»** Special packaging to protect against outer factors enabling easy storage,

**»** 33 mm. mobility zone

**»** Voltage : 48, 60, 80, 110, 190 V. DC 220 V. AC

**»** Bobbin Rotation / Hour : 240

**»** Weight : 5,5 kg.

**»** Two year actual guarantee.

[**Technical Drawing**](http://dapsan.com/uploads/Cizim_CL07.jpg)

