
Canlift CL-04



**CL-04  
Lift Landing Door Retering Cam**  
  
 **»** High quality and with technical features,  
**»** Convenient assembly and hardness,  
**»** Special packaging to protect against outer factors enabling easy storage,  
**»** 33 mm. mobility zone  
**»** Voltage : 48, 60, 80, 110, 190 V. DC 220 V. AC  
**»** Bobbin Rotation / Hour : 240  
**»** Weight : 5,5 kg.  
**»** Two year actual guarantee.

|  |  |
| --- | --- |
|  |  |
| [Technical Drawing](http://dapsan.com/uploads/Cizim_CL04.jpg)  [http://1.1.1.5/bmi/dapsan.com/uploads/Cizim_CL04.jpg](http://dapsan.com/uploads/Cizim_CL04.jpg) |  |