8003



FEATURES

• 4 mm galvanized sheet

• Polyamide guide shoe

• Supported by rubber

• 3 types for guides 5-9-16m

• Work speed max 1.2m/sc

**Technical Drawing**

