SKYGO2



**FEATURES**

• Fullfillment of lift directive 95/16/EC (EN 81-1 81-2)

• Engaging of the safety gear in both directions

• First cuts off the safety switch and than trips

• Overspeed governor with safety contact

• Configuration for machine room or shaft head possible

• Tensioning weight with safety contact

• Applicable for secondary installations and modernizations

• Pre-set according nominal speeds and sealed

• Fixing holes are completely compatible with other overspeed governors

• Mounting at almost everry lift type possible

• Easy installation and maintenance

• Test groove

• Detailed operating instructions

• Optional remote control unit

• Optional encoder ( Shaft Dia Ø 6-8 mm and Rabbet Dia Ø 30 mm )

**PRODUCT DIMENSIONS**

****